| PST SDK 6.0.0.0-272350a

Pause

Pause tracking

Pause the tracking system, stop producing tracking results and enter low-power mode. Tracking can be resumed with a subsequent call to PSTapi/Start.

Endpoint

      POST /PSTapi/Pause HTTP/1.1
      Host: address:port

Response

Returns a status message.

Verification table

Status Code | Content Example | Meaning
--- | --- | ---
200 | {"message":"Server on Pause"} | Success message
500 | {"message":"TrackerException: <...>"} | An other type of internal error