Loading...
Searching...
No Matches
SystemCheck

Check if the tracker is running correctly.

Endpoint

GET /PSTapi/SystemCheck HTTP/1.1
Host: address:port

Response

Returns one of the following status messages:

{"StatusMessage":"OK"}
{"StatusMessage":"NOT_INITIALIZED"}
{"StatusMessage":"DISCONNECTED"}
{"StatusMessage":"ERR_GENERAL"}
{"StatusMessage":"ERR_TIMEOUT"}
{"StatusMessage":"ERR_NOCAMS_FOUND"}
{"StatusMessage":"ERR_NOTENOUGHTCAMS_FOUND"}
{"StatusMessage":"ERR_INITERROR"}
{"StatusMessage":"ERR_CANNOT_START_CAMS"}
{"StatusMessage":"ERR_CANNOT_SETUP_CAMS"}

More information on the different status messages can be found in the PSTech::pstsdk::StatusMessage documentation.

StatusMessage Object

Key | Value Type | Description
--- | --- | ---
StatusMessage | string | The status of the tracker as a string object.

StatusMessage | Description
--- | ---
OK | The system is running OK.
NOT_INITIALIZED | Tracker failed to initialize correctly.
DISCONNECTED | The grabber has been disconnected.
ERR_GENERAL | Unspecified grabber error.
ERR_TIMEOUT | Grabber timeout error.
ERR_NOCAMS_FOUND | Grabber could not detect any cameras.
ERR_NOTENOUGHTCAMS_FOUND | Grabber could not detect sufficient cameras.
ERR_INITERROR | Grabber did not initialize correctly.
ERR_CANNOT_START_CAMS | Grabber could not start cameras.
ERR_CANNOT_SETUP_CAMS | Grabber failed setting up cameras.

Example

{"StatusMessage":"OK"}

Verification table

Status Code | Content Example | Meaning
--- | --- | ---
200 | JSON payload | Success message
500 | {"message":"TrackerException: <...>"} | An other type of internal error