| PST SDK 6.0.0.0-272350a

restserver.c

This example can be found in `examples\c\restserver\restserver.c`.

This example shows how to enable the REST server using the PST SDK. The REST server enables network-based access to the PST Tracker using the HTTP protocol. GET and POST requests can be made to the server to send and receive data and change parameters. The REST interface offers a programming language independent interface to the PST Tracker. Besides accessing the REST server directly using a browser, a networking library like Curl can be used to interface with the server programatically.

When compiling and running this example, please make sure that the required dependencies can be found by the executable (e.g. by copying the `Redist` directory into the build directory. When the PST SDK has been installed through the PST Software Suite installer the Redist folder can be found in the Development folder.).

#ifdef WIN32
#include <windows.h>
#else
#include <unistd.h>
#endif
/*
* Define handler functions required to ensure a clean shutdown of the PST Tracker
* when the application is terminated.
*/
static void Exithandler(int sig);
#ifdef WIN32
BOOL WINAPI ConsoleHandler(DWORD CEvent)
{
Exithandler(CEvent);
return TRUE;
}
#endif
/* End of handler functions */
#include "pstsdk_c.h"
#include <stdio.h>
#include <stdlib.h>
#include <signal.h>
/*
* Implement the exit handler to shut-down the PST Tracker connection on application termination.
*/
static void Exithandler(int sig)
{
pst_sdk_disable_rest_server();
pst_sdk_shutdown();
exit(0);
}
// Print the last error message.
void PrintLastErrorMessage()
{
char* last_error_message = NULL;
EPstErrorStatus error_status = pst_alloc_and_get_last_error_message(&last_error_message);
if (error_status != PST_ERROR_STATUS_OK)
{
last_error_message = "Failed to allocate memory error.";
}
printf("last error message: %s \n", last_error_message);
pst_free(last_error_message);
}
// Check error status and shutdown tracker upon error.
void CheckErrorCode(EPstErrorStatus status)
{
if (status != PST_ERROR_STATUS_OK)
{
PrintLastErrorMessage();
pst_sdk_shutdown();
exit(status);
}
}
int main(int argc, char *argv[])
{
// Register the exit handler with the application
#ifdef WIN32
SetConsoleCtrlHandler((PHANDLER_ROUTINE)ConsoleHandler, TRUE);
#else
signal(SIGTERM, Exithandler);
signal(SIGKILL, Exithandler);
signal(SIGQUIT, Exithandler);
signal(SIGINT, Exithandler);
#endif
PstTracker ctracker;
#ifdef WIN32
// Create an instance of the Tracker object using the default configuration path and file names.
CheckErrorCode(pst_tracker_init(&ctracker));
#else
// On Linux, specify the type of grabber that needs to be used as the last parameter:
// "basler_ace" for PST HD or "basler_dart" for PST Pico
CheckErrorCode(pst_tracker_init4(&ctracker, "", "config.cfg", "models.db", argv[1]));
#endif
// Start the tracker server.
CheckErrorCode(pst_tracker_start(&ctracker));
// Enable the REST server. To check if the REST server is started correctly, browse to
// http://localhost:7278/PSTapi/SystemCheck
// In order to use 127.0.0.1 an an address on Windows 7, execute the following command
// on an elevated command prompt to allow communication to this address:
// "netsh http add urlacl url=http://127.0.0.1:7278/ user=EVERYONE listen=yes delegate=no"
CheckErrorCode(pst_sdk_enable_rest_server("localhost", "7278", 3000));
printf("PST REST server enabled. See the PST SDK Manual for example commands.\n");
// Wait for one minute before terminating this application.
#ifdef WIN32
Sleep(60000);
#else
sleep(60);
#endif
// Disable the REST server
pst_sdk_disable_rest_server();
// Make sure that the connection to the PST Tracker is shut down properly.
pst_tracker_destroy(&ctracker);
return 0;
}